OBSOLETE Patch-ID# 112488-04
Keywords: Sun Fire 15K SMS
Synopsis: Obsoleted by: 112488-05 SMS 1.2: domain isolation not seen when degrading domain using setbus
Date: May/03/2002

Solaris Release: 8 9

SunOS Release: 5.8 5.9

Unbundled Product: System Management Services

Unbundled Release: 1.2

Xref: 

Topic: SMS 1.2: domain isolation not seen when degrading domain using setbus

Relevant Architectures: sparc

BugId's fixed with this patch: 4525385 4531458 4533839 4548741 4587418 4587605 4599570 4614186 4615412 4616748 4616754 4617503 4619131 4619143 4621354 4622129 4630077 4633429 4635057 4635471 4635496 4636719 4638620 4638977 4640847 4649452 4649862

Changes incorporated in this version: 4635057 4635471 4635496 4636719 4638620 4638977 4640847 4649452 4649862

Patches accumulated and obsoleted by this patch: 

Patches which conflict with this patch: 

Patches required with this patch: 

Obsoleted by: 

Files included with this patch: 

/opt/SUNWSMS/SMS1.2/bin/hpost
/opt/SUNWSMS/SMS1.2/bin/redx
/opt/SUNWSMS/SMS1.2/lib/libxcpost.so

Problem Description:

4635057 Post does not correctly auto connect cassettes on the hpci for the demios card
4635471 wfail misdiagnoses ecache UE recordstops.
4635496 libxcpost change required for MaxCPU DR
4636719 AMX/RMX RStop clear should not leave port error indicators masked
4638620 FAIL BBC may not fail correct ports
4638977 wcp_wci_read()/xcp_wci_write() can cause WCI pull_stop
4640847 wfail display of SDI local first errors causes confusion
4649452 deleteboard in degraded mode causes DStop; recovery fails; setbus normal fails
4649862 Remove up-level warning on Ethernet hub
 
(from 112488-03)
 
4525385 hpost needs to understand new LPOST version scheme
4548741 xcp_poll_server misses detection of OBP entry
4587605 AXQ revs 6.0 and 6.1 are interpreted incorrectly.
4599570 Running hpost -H on attach-ready IO0 causes DStop
4616748 Sequential hpost -H,f on same L1 board causes RStop in domain
4621354 Some degraded bus configurations can break SC interrupt delivery.
4622129 EXB domain masks not configured correctly in CP loopback mode
4633429 pcs_poll_servers(): exiting poll flow on PROC_INFO_NEXT_SCTEST
 
(from 112488-02)
 
4533839 Write/read-compare on Ethernet hub fails intermittently
4630077 Change dcu_features to a level-2 (service) command
 
(from 112488-01)
 
4531458 domain isolation not seen when degrading a domain using setbus
4587418 hpost -Q does not init all CPU state
4614186 dr in of unused exp causes DStop when target domain is degraded
4615412 hpost CPU timeouts in ProDomAdvR1 during hpost -H
4616754 hpost ignores the "attach-ready" state of L1 boards
4617503 hpost -Q needs to update DCB cbase and cbnd values
4619131 hpost needlessly locks all expanders in a domain when testing a single board
4619143 chunk list construction must use MADR information

Patch Installation Instructions:
--------------------------------
 
For Solaris 2.0-2.6 releases, refer to the Install.info file and/or
the README within the patch for instructions on using the generic
'installpatch' and 'backoutpatch' scripts provided with each patch.
 
For Solaris 7-8 releases, refer to the man pages for instructions
on using 'patchadd' and 'patchrm' scripts provided with Solaris.
Any other special or non-generic installation instructions should be
described below as special instructions.  The following example
installs a patch to a standalone machine:
 
        example# patchadd /var/spool/patch/104945-02
 
The following example removes a patch from a standalone system:
 
        example# patchrm 104945-02
 
For additional examples please see the appropriate man pages.
 
See Also:  System Management Services (SMS) 1.2 Installation Guide and
           Release Notes, Part No. 816-2529-10
           Chapter 1, Patches

Special Install Instructions:
-----------------------------
 
Follow these steps when installing on the SC:
1. Record which SC is the main SC.
2. Stop the SMS processes on both SC's simultaneously.
        /etc/init.d/sms stop
3. Install the patch on both SC's.
4. Start the SMS processes on the previous main SC first.
        /etc/init.d/sms start
5. After all the sms processes have started (i.e. you're able to run the
   showenvironment command and get all the system's status),
   start the SMS processes on the Spare SC next.
        /etc/init.d/sms start

README -- Last modified date:  Monday, May 20, 2002

