Fibre Channel Errors |

Fibre Channel errors are represented by red links and the letters 'fc,' also in red. Fibre Channel errors indicate that CRC or ITW were found at either end of the link in red.

Fibre Channel errors are usually intermittent and do not represent a hard failure.
When a hard failure occurs, such as when a switch port has gone offline, fibre channel counters are ignored.

See Also:

- Display Topology Feature Hints
- MPxIO Errors
- Topology Icons