This page is used to start volume verification on Sun T3, Sun 6020 and Sun 6120 storage arrays. This option will execute volume verify continuously on all arrays at the selected rate. Volumes are verified one at a time on a rotational basis.
'Kill Verify' can be used to abort these operations on each array.
The 'Device Summary' page displays each monitored array with information about 'vol verify'.
The 'Execution Rate' for the volume verification determines the impact on I/O access to the array.
Selecting an 'Execution Rate' of 1 will take longer to verify the volume but will have less effect on I/O.