[util.ps]
name=Run unix ps
desc=Process Status
path=bin/ps
syntax=-f#c=1
syntax_name=All_Processes Full_listing
fixed=-e

[t3.changeArrayPwd]
name=Change Array passwords
desc=This command will change all Storage Array passwords for a 3900/6900
path=sysbin/changeArrayPasswords
solution=se,se2
hide_args=1
syntax=-o#p20 -n#p20 -f#c0
syntax_name=Old_Password New_Password Force_new

[t3.testt3]
name=Retrieve tokens from a Array
desc=Enter IP Address and a 0 or 1 for the first or second enclosure (Partner Group)
path=bin/testt3
options=<IP> 0|1
syntax=#t20 #s0|1=0 #selemprop|sysprop|system|fru|frudata|fruprop|portprop|slice|volprop|vol|lun|loopinfo|sysdata
syntax_name=IP Enclosure# Page
default=<IP> 0

[t3.command]
name=Run Commands on Array
desc=Run command using telnet (fru list, fru stat etc..)
path=bin/t3command
hide_args=1
syntax=-i#t20 -p#p20 -c#sfru+list|fru+stat|port+list|sys+list|vol+list|vol+stat|volslice+list -a#t30 
syntax_name=IP Password Command Argument

[util.config_solution]
name=Create SE-Series snapshot
path=sysbin/config_solution
solution=se,se2
syntax=-m#s3900SL|3910|3960|6320|6910|6910SL|6960|6960SL=3910  -p#p20 -i#t20  -h#c=0 
syntax_name=Model VE_Password Subnet_Prefix Help
timeout=300


