SunMC Provider |

The SunMC Provider enables the Storage Automated Diagnostic Environment to send actionable events and monitoring topologies to the SunMC Console, which displays the alarms and alert text. SunMC information is similar and compatible with Sun Remote Services (SRS). SunMC can send information to SRS, in which case the SRS Provider need not be activated in the Storage Automated Diagnostic Environment. This feature needs to be enabled and configured before devices are discovered for topology to be properly displayed in the SunMC Console.

To set up the SunMC Module, complete the following steps:

- pkgadd SUNWesraa on your host running the SunMC agent.

- SUNWesraa can be found in SUNWstade/System/SunMC.

- Load the rasagent module from the SunMC Console.
- Add the IP address of the StorADE host in the rasagent module from the SunMC Console.
- Enable the rasagent module from the SunMC Console.

To set up the SunMC Provider, complete the required fields:

- Enable the Active checkbox.
- Type the SunMC console IP address.
- Specify the port number. The default is 162.
- Specify the number of hours for heartbeat frequency.

See Also:

- Email Provider
- SRS Net Connect Provider
- SNMP Provider
- SRS Provider
- SSRR Provider
- SAE Provider