This function can be used to:
- Generate a list of required patches for a storage system.
- Install these patches on each component of the storage system.
WARNING:
- Disk drive upgrades with controller firmware 3.2 or greater no longer requires ALL I/O to the array be quiesced.
- Disk drive upgrades below controller firmware 3.2 requires ALL I/O to the array be quiesced.
NOTE:
- Turn-off device monitoring to avoid false events during upgrade.
- Selecting a device will install all patches listed for that device. The Service processor does not allow selection of individual patches.