//
// Copyright 2000-2002 Sun Microsystems, Inc.  All rights reserved.
// Use is subject to license terms.
//

#pragma ident	"@(#)esmd_tuning.txt	1.38	03/05/21 SMI"

*
*            ESMD Tunable Thresholds and Intervals
*
** Note: Only Sun's knowledgeable engineers are authorized to make changes.
*

*
*-Monitoring Interval in Seconds
*
    mon_temp_interval      = 60
    mon_node_temp_interval = 60
    mon_proc_temp_interval = 10
    mon_volt_interval      = 60
    mon_device_interval    = 60
    mon_state_interval     = 30
    mon_config_interval    = 30
    mon_frutime_interval   = 60

*
*-Response Time in Seconds
*
    rsp_comp_exceed_op_limit = 180
    rsp_proc_over_temp       = 180

*
*-Cabinet Temperature Monitoring Tuner
*
** Thermal Limits
*
    cab_ambient_low_warn         = 5.0
    cab_ambient_optimum          = 15.0
    cab_ambient_high_warn        = 25.0
    cab_ambient_high_crit        = 35.0
    cab_ambient_overlimit        = 40.0
    cab_ambient_sensor_delta_max = 6.0

*
** Temperature Change Cushion
*
    cab_normal_temp_event_cushion   = 5.0
    cab_abnormal_temp_event_cushion = 2.0
    cab_boundry_temp_cushion = 0.5
    cab_fan_reset_temp_cushion = 5.0

*
*-System Control Board Temperature Monitoring Tuner
*
** Thermal Limits
*
   scb_asic_high_warn        = 85.0
   scb_asic_high_crit        = 95.0
   scb_asic_overlimit        = 105.0
   scb_proximity_high_warn   = 45.0
   scb_proximity_high_crit   = 50.0
   scb_proximity_overlimit   = 55.0
   scb_powersupply_high_warn = 70.0
   scb_powersupply_high_crit = 75.0
   scb_powersupply_overlimit = 80.0

*
*-Centerplane Support Board Temperature Monitoring Tuner
*
** Thermal Limits
*
   csb_asic_high_warn      = 85.0
   csb_asic_high_crit      = 95.0
   csb_asic_overlimit      = 105.0
   csb_proximity_high_warn = 45.0
   csb_proximity_high_crit = 50.0
   csb_proximity_overlimit = 55.0
 
*
*-Centerplane Board Temperature Monitoring Tuner
*
** Thermal Limits
*
   cpb_asic_high_warn = 70.0
   cpb_asic_high_crit = 80.0
   cpb_asic_overlimit = 85.0
 
*
*-Expander Board Temperature Monitoring Tuner
*
** Thermal Limits
*
   exb_asic_high_warn      = 85.0
   exb_asic_high_crit      = 95.0
   exb_asic_overlimit      = 105.0
   exb_asic_III_high_warn  = 70.0
   exb_asic_III_high_crit  = 80.0
   exb_asic_III_overlimit  = 85.0
   exb_proximity_high_warn = 45.0
   exb_proximity_high_crit = 50.0
   exb_proximity_overlimit = 55.0
 
*
*-CPU Board Temperature Monitoring Tuner
*
** Thermal Limits
*
   cpub_asic_high_warn = 85.0
   cpub_asic_high_crit = 95.0
   cpub_asic_overlimit = 105.0
   cpub_proc_high_warn = 88.0
   cpub_proc_high_crit = 93.0
   cpub_proc_overlimit = 98.0
   cpub_proc_plus_high_warn = 88.0
   cpub_proc_plus_high_crit = 93.0
   cpub_proc_plus_overlimit = 98.0

*
*-PCI Board Temperature Monitoring Tuner
*
** Thermal Limits
*
   pcib_asic_high_warn        = 85.0
   pcib_asic_high_crit        = 95.0
   pcib_asic_overlimit        = 105.0
   pcib_powersupply_high_warn = 70.0
   pcib_powersupply_high_crit = 75.0
   pcib_powersupply_overlimit = 80.0

*
*-hPCI+ Board Temperature Monitoring Tuner
*
** Thermal Limits
*
   hpcix_asic_high_warn        = 85.0
   hpcix_asic_high_crit        = 95.0
   hpcix_asic_overlimit        = 105.0
   hpcix_asic_III_high_warn    = 70.0
   hpcix_asic_III_high_crit    = 80.0
   hpcix_asic_III_overlimit    = 85.0
   hpcix_powersupply_high_warn = 70.0
   hpcix_powersupply_high_crit = 75.0
   hpcix_powersupply_overlimit = 80.0

*
*-Dual CPU Board Temperature Monitoring Tuner
*
** Thermal Limits
*
   mxtb_asic_high_warn = 90.0
   mxtb_asic_high_crit = 100.0
   mxtb_asic_overlimit = 105.0
   mxtb_proc_high_warn = 88.0
   mxtb_proc_high_crit = 93.0
   mxtb_proc_overlimit = 98.0
   mxtb_proc_plus_high_warn = 88.0
   mxtb_proc_plus_high_crit = 93.0
   mxtb_proc_plus_overlimit = 98.0

*
*-WIB PCI Board Temperature Monitoring Tuner
*
** Thermal Limits
*
   wpcib_asic_high_warn = 80.0
   wpcib_asic_high_crit = 95.0
   wpcib_asic_overlimit = 105.0
   wpcib_asic_III_high_warn = 70.0
   wpcib_asic_III_high_crit = 80.0
   wpcib_asic_III_overlimit = 85.0
 
*
*-System Control Board Voltage Monitoring Tuner
*
** Voltage Limits
*
   scb_1.5vdc_low_min  = 1.4
   scb_1.5vdc_high_max = 1.6
   scb_3.3vdc_low_min  = 3.0
   scb_3.3vdc_high_max = 3.5

   scb_3.3hk_low_min   = 3.0
   scb_3.3hk_high_max  = 3.5
   scb_5.0vdc_low_min  = 4.75
   scb_5.0vdc_high_max = 5.25
   scb_+12vdc_low_min  = 11.4
   scb_+12vdc_high_max = 12.6
   scb_-12vdc_low_min  = -12.6
   scb_-12vdc_high_max = -11.4

   scb_1.5vcnvtr_percent   = 0.50
   scb_3.3vcurrent_percent = 0.50
   scb_5.0vcurrent_percent = 0.50

*
*-System Control IO Board Voltage Monitoring Tuner
*
   scper_3.3vdc_low_min  = 3.0
   scper_3.3vdc_high_max = 3.5
   scper_3.3hk_low_min   = 3.0
   scper_3.3hk_high_max  = 3.5
   scper_5.0vdc_low_min  = 4.75
   scper_5.0vdc_high_max = 5.25
   scper_+12vdc_low_min  = 11.4
   scper_+12vdc_high_max = 12.6

*
*-Centerplane Support Board Voltage Monitoring Tuner
*
** Voltage Limits
*
   csb_1.5vdc_low_min  = 1.4
   csb_1.5vdc_high_max = 1.6
   csb_2.5vdc_low_min  = 2.3
   csb_2.5vdc_high_max = 2.7
   csb_3.3vdc_low_min  = 3.0
   csb_3.3vdc_high_max = 3.5
   csb_3.3hk_low_min   = 3.0
   csb_3.3hk_high_max  = 3.5
 
*
*-Expander Board Voltage Monitoring Tuner
*
** Voltage Limits
*
   exb_1.5vdc_low_min  = 1.4
   exb_1.5vdc_high_max = 1.6
   exb_2.5vdc_low_min  = 2.3
   exb_2.5vdc_high_max = 2.7
   exb_3.3vdc_low_min  = 3.0
   exb_3.3vdc_high_max = 3.5
   exb_3.3hk_low_min   = 3.0
   exb_3.3hk_high_max  = 3.5
 
*
*-CPU Board Voltage Monioring Tuner
*
** Voltage Limits
*
   cpub_1.5vdc_low_min  = 1.4
   cpub_1.5vdc_high_max = 1.6
   cpub_3.3vdc_low_min  = 3.0
   cpub_3.3vdc_high_max = 3.5
   cpub_core_percent    = 0.20

*
*-PCI Board Voltage Monitoring Tuner
*
** Voltage Limits
*
   pcib_1.5vdc_low_min  = 1.4
   pcib_1.5vdc_high_max = 1.6
   pcib_3.3vdc_low_min  = 3.0
   pcib_3.3vdc_high_max = 3.5
   pcib_3.3hk_low_min   = 3.0
   pcib_3.3hk_high_max  = 3.5
   pcib_5.0vdc_low_min  = 4.75
   pcib_5.0vdc_high_max = 5.25
   pcib_+12vdc_low_min  = 11.4
   pcib_+12vdc_high_max = 12.6
   pcib_-12vdc_low_min  = -12.6
   pcib_-12vdc_high_max = -11.4

   pcib_1.5vcnvtr_percent   = 0.50
   pcib_3.3vcurrent_percent = 0.50
   pcib_5.0vcurrent_percent = 0.50

*
*-hPCI+ Board Voltage Monitoring Tuner
*
** Voltage Limits
*
   hpcix_1.5vdc_low_min  = 1.4
   hpcix_1.5vdc_high_max = 1.6
   hpcix_2.5vdc_low_min  = 2.3
   hpcix_2.5vdc_high_max = 2.7
   hpcix_3.3vdc_low_min  = 3.0
   hpcix_3.3vdc_high_max = 3.5
   hpcix_3.3hk_low_min   = 3.0
   hpcix_3.3hk_high_max  = 3.5
   hpcix_5.0vdc_low_min  = 4.75
   hpcix_5.0vdc_high_max = 5.25
   hpcix_+12vdc_low_min  = 11.2
   hpcix_+12vdc_high_max = 12.8
   hpcix_-12vdc_low_min  = -13.0
   hpcix_-12vdc_high_max = -11.0

*
*-Dual CPU Board Voltage Monioring Tuner
*
** Voltage Limits
*
   mxtb_1.5vdc_low_min  = 1.4
   mxtb_1.5vdc_high_max = 1.6
   mxtb_3.3vdc_low_min  = 3.0
   mxtb_3.3vdc_high_max = 3.5
   mxtb_3.3hk_low_min   = 3.0
   mxtb_3.3hk_high_max  = 3.5
   mxtb_core_percent    = 0.05

*
*-WIB PCI Board Voltage Monitoring Tuner
*
** Voltage Limits
*
   wpcib_+12vdc_low_min  = 11.4
   wpcib_+12vdc_high_max = 12.6
   wpcib_-12vdc_low_min  = -12.6
   wpcib_-12vdc_high_max = -11.4
   wpcib_3.3hk_low_min   = 3.0
   wpcib_3.3hk_high_max  = 3.5
   wpcib_3.3vdc_low_min  = 3.0
   wpcib_3.3vdc_high_max = 3.5
   wpcib_1.5vdc_low_min  = 1.4
   wpcib_1.5vdc_high_max = 1.6
   wpcib_2.5vdc_low_min  = 2.3
   wpcib_2.5vdc_high_max = 2.7
   wpcib_5.0vdc_low_min  = 4.75
   wpcib_5.0vdc_high_max = 5.25
   wpcib_1.5vdc_par_low_min  = 1.42
   wpcib_1.5vdc_par_high_max = 1.57
   wpcib_3.3vdc_par_low_min  = 3.13
   wpcib_3.3vdc_par_high_max = 3.47
