OBSOLETE Patch-ID# 115846-03
Keywords: sun fire v440 netra 440
Synopsis: Obsoleted by: 115846-04 Hardware/PROM: Sun Fire V440 and Netra 440 Flash PROM Update
Date: Jun/01/2004


Install Requirements: Additional instructions may be listed below                      
                      
Solaris Release: 8 9

SunOS Release: 5.8 5.9

Unbundled Product: Hardware/PROM
    NOTE: If you have the frame buffer Raptor GFXP -04 REV 50
          (part 370-3753-04), you *must* install patch 110126-03 to
          upgrade the FCode in the card **BEFORE** you can do the
          firmware update. Revisions -05 and up of the frame buffer
          are not affected.
	  Failure to install the frame buffer patch (110126-03)
	  will cause "FATAL" resets after the firmware update.
    NOTE: This utility is *not* OS-dependent.  The list of releases shown
          under the "Solaris Release" and "SunOS Release" sections may not 
          be complete: The absence of a valid Solaris Release or SunOS  
          Release from the lists above does not preclude the installation 
          of this patch against the hardware.


Unbundled Release: OBP_4.13.0, POST_4.13.0, OBDIAG_4.13.0

Xref: 

Topic: 

Relevant Architectures: sun fire v440, netra 440

BugId's fixed with this patch: 4791537 4802415 4804991 4825521 4829098 4829331 4834606 4841495 4849305 4850283 4850344 4850706 4852206 4853436 4854134 4856209 4856347 4857933 4859625 4861512 4861585 4862646 4862684 4864627 4864985 4870753 4872592 4876043 4879743 4882093 4883792 4883794 4886234 4890068 4890075 4890305 4893067 4893726 4895659 4897231 4898596 4901202 4902931 4910442 4920572 4930316 4932215 4942884 4946063 4948794 4949133 4953893 4955331 4965742 4969997 4972307
NOTE:
BugIds fixed in previous patches: 
4.10.14
-------
4870753, 4879743, 4893067, 4883792, 4883794, 4898596, 4909779, 4946063
4.10.10
-------
4909779, 4870753, 4879743, 4893067, 4872592, 4883792, 4898596, 4883794

Changes incorporated in this version: 

Patches accumulated and obsoleted by this patch: 

Patches which conflict with this patch: 

Patches required with this patch: 110126-03 or greater
NOTE: see frame buffer note above.

Obsoleted by: 

Files included with this patch: 

				README.115846-03, 802-3233-25.ps,
				flash-update-SunFire440-02,
				unix.flash-update.README, copyright
				unix.flash-update.SunFire440.sh*,
flash-update-SunFire440-latest, 

Problem Description:

BugID		Synopsis
-----   	--------
4.13.0
------
4791537          after hitting breakpoint obp will not proceed further with 'step' or 'go'
4829098          corrupt nvram is not reported, crc is silently re-written
4841495          local-mac-address properties not created correctly in net devices.
4850344          fix 4.x and 4.11 version of lsi1030.fth message to match 4.10 version
4852206          OBP using Tomatillo SRAM potentially clobbered by POST
4856347          ENWS power up FAIL WARNING: Last shutdown is later than time on tod chip
4857933          checksum library Makefile missing dependency and rule for sparcv9 target dir
4861512          pcf8584 i2c probing code needs to retry.
4861585          ASR keylist should include onboard PCI devices.
4862646          USB keyboard FCode should not assume interface number
4862684          WARNING:Failed to open device(/pci@1e,600000/isa@7/i2c@0,320/gpio...
4864627          OPS need rmc-log node to clear rmc.
4876043          remove bogus rmc-log node
4802415          obp needs to warn that booting after running obdiag prevents OS from coming up
4804991          "MMU Miss" is generated when "reset -x" is issued and boot-file is set to kadb
4825521          XXIIRR  ffaaiilleedd messaged displayed if XIR is sent during opb initialization
4829331          Running OBDiag with disg-script = 'none' causes an extra reset
4864985          do faster mapping using on-demand generation of translations and forth assembler
4870753          Transfer SCC card from Enchilada to Chalupa, sets auto-boot? to false
4879743          OBP input/outpu-file defaults changed to ttya; Examine return to screen/keyboard
4882093          asr fixes
4890068          Implement enhanced PHY reset code for BGE devices
4890075          Version check for BGE errata application does not work
4890305          Clean up nits in the common workspace
4893067          add support for JEDEC DDR v1.0 SPD
4893726          Updating OBP from Solaris with keyswitch=LOCKED results in unclear message
4901202          Part number list for ENTS/ENWS flash update need to be updated.
4834606          make depend under obp/dev/scsi/adapters/lsi1030 fails
4897231          OBP downgrade to 4.7.5 causes 20 minute hang during reset
4910442          POST output fails to be directed to RSC
4920572          support explicit nvram partitions
4932215          cannot update Fujitsu Flash.
4946063          PCI address parity error causes sudden sys-reset.
4948794          Chalupa 19" support for fiesta OBP gate
4953893          New Motherboard and Centerplane Partnumbers will cause Flash-update to fail.
4969997          OBP needs to support JP3.2 Errata 102, 104
4849305          POST fails with "IO-Bridge unit 1 sram      test" error
4850283          i-cache parity functional test failure
4850706          Fast ecc, system ecc test errors
4853436          POST AFT mapping is incorrect
4854134          POST hangs if mixed speed cpu modules are populated
4856209          POST uses the word "errors" in test name causing OPS tests to fail
4859625          Implement FWARC 2003/258.
4872592          POST L2 cache errors on JP3.1 processors
4883792          POST gives false error when using CPU speed entry from rw section
4883794          Printing fru information is painfully slow
4886234          Top level make does not detect changed files
4895659          POST checksum test does not do complete test
4898596          POST needs to dump AFSR and AFAR register content on FATAL event during POST
4902931          Some tomatillo errors are NOT enabled in POST
4930316          Enable diagnostics as a default for VSP servers.
4942884          POST directory structure updates and code cleanup
4949133          Add gemini support
4955331          Chalupa 19" banner name support with fiesta POST gate
4965742          watchdog timeout in POST
4972307          chalupa build fails
 
4.10.14
-------
4870753		Transfer SCC card from Enchilada to Chalupa, sets auto-boot? to false
4879743		OBP input/outpu-file defaults changed to ttya; Examine return to screen/keyboard
4893067		add support for JEDEC DDR v1.0 SPD
4883792		POST gives false error when using CPU speed entry from rw section
4883794 	Printing fru information is painfully slow
4898596		POST needs to dump AFSR and AFAR register content on FATAL event during POST
4909779		Debug switch dropin-checksum? inhibits flash update recovery
4946063		PCI address parity error causes sudden sys-reset.
 
4.10.10
-------
4909779  	Debug switch dropin-checksum? inhibits flash update recovery
4870753  	Transfer SCC card from Enchilada to Chalupa, sets auto-boot? to false
4879743  	OBP input/outpu-file defaults changed to ttya; Examine return to screen/keyboard
4893067  	add support for JEDEC DDR v1.0 SPD
4872592  	POST L2 cache errors on JP3.1 processors
4883792  	POST gives false error when using CPU speed entry from rw section
4898596  	POST needs to dump AFSR and AFAR register content on FATAL event during POST
4883794  	Printing fru information is painfully slow

Patch Installation Instructions:
===============================
 
 
Intro
-----
 
    This README is intended for users who wish to upgrade the firmware
    in their Sun Fire V440 or Netra 440.
 
 
Summary of the Patch Installation Process:
------------------------------------------
 
The installation shall comprise of the following steps
 
1)  Determine the system's current Flash PROM firmware revision.
 
2)  Compare the current Flash PROM firmware revision with the available or 
    latest Flash PROM firmware revisions.
 
3)  If the current Flash PROM firmware revision is lower than the latest
    available firmware revision in this patch, then proceed to the next step. 
    If NOT, STOP: DO NOT CONTINUE.
 
4)  Prepare the system for the Flash PROM update
 
5)  Running the Flash PROM Utility
 
6)  Verifying successful Flash PROM Update
 
7)  Restoring the system
 
8)  Resume operations
 
 
Patch Installation instructions (in detail):
============================================
 
The required steps are explained in greater detail below.
 
1)  Determine the System's Current Firmware Revisions
    -------------------------------------------------
 
    While the OS is running the following command may be used to
    determine the current system firmware revisions;
 
        /usr/sbin/prtconf -V
        or
	/usr/platform/sun4u/sbin/prtdiag -v | grep OBP
 
    The firmware revisions may also be determined from the PROM monitor's
    "ok" prompt with the following command;
 
	.version
 
2)  Compare the current Flash PROM firmware revision with the available or 
    latest Flash PROM firmware revisions.
 
    Compare the output of the OBP line in the "prtdiag -v" or "prtconf -V"
    output. Find the revision number and compare with the revision on the
    entries below that of the "flash-update-SunFire440-latest" line
 
      Available Firmware Revisions
      ----------------------------
 
-LATEST flash-update-SunFire440-latest
	OBP  4.13.0 created 2004/01/19 18:28 Sun Fire V440,Netra 440
	POST 4.13.0 2004/01/16 12:35 
 
-02     flash-update-SunFire440-02
	OBP  4.10.14 created 2003/11/19 14:09 Sun Fire V440
	POST 4.10.12 2003/10/15 22:33 
 
3)  Is the UPGRADE NECESSARY?
 
    If the current Flash PROM revision matches the version numbers given under
    the flash-update-SunFire440-latest line, then STOP Here. This UPGRADE IS NOT
    NECESSARY.
 
    If the current Flash PROM firmware revision is lower than the latest
    firmware revision in this patch, then proceed to the next step.
 
4) Preparing the System
   ---------------------
 
  a) As root, copy the latest "flash-update" files from the directory
     containing the patch to the root directory as follows:
 
     # cp flash*latest  /
     # chmod 755 /flash-update*
 
     In order to boot the binary, it must be located within the root
     partition.  If it is not already located within the root partition
     then move it to /.  If the binary is already located elsewhere 
     within the root partition then note the exact filepath so that the
     binary can be booted later.
 
  b) As root, exit the OS such that the system returns to the PROM's "ok"
     prompt: 
 
     # halt
 
       ok
 
  c) Jumper J4205 is factory-set so that the flash PROM is write-enabled.
     There is no need to switch the jumper before flash updating; however,
     you must ensure that the keyswitch is in the Power-on or Diagnostics
     position.  When the key switch is in the locked position the flash
     PROM is write protected.
 
5)  Running the Flash Update Utility
    --------------------------------
     ** NOTE **  If the flash update completes normally then the values
     contained within the system's Non-Volatile RAM (NVRAM) configuration
     variables will be retained.  However, if the update process is some-
     how interrupted then it is possible that any non-default values
     contained in NVRAM will be lost.  For this reason it is recommended
     that you note down on paper the contents of any NVRAM configuration
     variable which has been customized so that they may be manually
     restored at a later time, if necessary.  (Use the PROM's "printenv"
     command to list the variables and their values.)
 
  a) The system should now display the PROM monitor's "ok" prompt.
     Now boot the Flash update utility as given below:
 
     CAUTION: Do not boot/run revisions lower than the latest unless you
	      are absolutely sure that that is what you want to do!
 
     ok boot disk /flash-update-SunFire440-latest
 
     NOTE: If your system's boot device is not "disk" then you will
           have to specify the appropriate devalias (e.g. disk2).
           If the binary is located in a location other than / then
           provide the entire filepath after the boot device.
 
     Answer the questions as prompted by the utility. 
 
 
+++++++++++++++++++++ example Flash update follows ++++++++++++++++++++++++
++++++++ Note that this is an example only.  Much of the information ++++++
++++++++ which is displayed by your system will be different from    ++++++
++++++++ what is shown below.                                        ++++++
+++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
 
 
Standalone Flash PROM Update Utility, Rev. 2.7
                        Ultra(tm) 1
                        Ultra(tm) 2
                        Ultra(tm) 5/10
                        Ultra(tm) 30
                        Ultra(tm) 60 / E220R
                        Ultra(tm) 80 / E420R
                        Ultra(tm) Enterprise(tm) 250
                        Ultra(tm) Enterprise(tm) 450
			Sun Blade(tm) 100
			Sun Blade(tm) 1000
			Sun Fire (tm) 280R
			Netra(tm) T4 
			Sun Fire (tm) V880
			Sun Fire (tm) V440
 
This utility allows you to interactively update the firmware
revisions in specific system Flash PROM components.
 
Type h for help, q to quit, Return or Enter to continue:
 
Every precaution should be taken to prevent the loss of system
power during the Flash PROM programming process!
 
Type h for help, q to quit, Return or Enter to continue:
 
 
       Firmware Release(s)                Firmware Release(s)
 Currently Existing in the System      Available for Installation  /  Install?
---------------------------------- -------------------------------------------
OBP 4.10.5  2003/05/22 13:58         OBP 4.10.10 2003/08/29 06:25          no
POST 4.10.5 2003/05/22 18:02         POST 4.10.9 2003/08/05 13:15          no
 
Type sa if you wish to select all available firmware releases for
installation.  Type h for help, quit to exit, or cont to continue: sa
 
 
       Firmware Release(s)                Firmware Release(s)
 Currently Existing in the System      Available for Installation  /  Install?
---------------------------------- -------------------------------------------
OBP 4.10.5  2003/05/22 13:58         OBP 4.10.10 2003/08/29 06:25         YES 
POST 4.10.5 2003/05/22 18:02         POST 4.10.9 2003/08/05 13:15         YES 
 
Type sa if you wish to select all available firmware releases for
installation.  Type h for help, quit to exit, or cont to continue: cont
 
 
The Flash programming process is about to begin.
 
Type h for help, q to quit, Return or Enter to continue:
 
Erasing the top half of the Flash PROM.
Programming OBP into the top half of the Flash PROM.
Verifying OBP in the top half of the Flash PROM.
 
Erasing the bottom half of the Flash PROM.
Programming OBP into the bottom half of Flash PROM.
Verifying OBP in the bottom half of the Flash PROM.
 
Erasing the top half of the Flash PROM.
Programming POST into the top half of Flash PROM.
Verifying POST in the top half of the Flash PROM.
 
Programming was successful.
 
Resetting ...
 
 
+++++++++++++++++++++ example Flash update ends ++++++++++++++++++++++++++
 
  Once the PROM's banner reappears then use the Stop-A keys (or Break
  key, if running from a serial line) to abort the auto-boot sequence
  if the system begins to boot.
 
6)  Verifying successful Flash PROM Update
 
    Verify from the results of the .version command that the OBP
    version matches the OBP version given above under the
    flash-update-SunFire440-latest entry in Step 2.
 
7)  Resume operations
 
    a) Allow the system to auto-boot, by issuing a "go" command or issue 
       the boot command for your environment.
 
    b) Once the system has rebooted you may wish to remove the Flash Update
       binaries and documents since they will no longer be needed.
 
       # rm /flash-update*
 
    c) Remember to remove the files from their original location if
       they were not extracted directly into the root directory.
 
 
*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-

Special Install Instructions:
----------------------------- 
 
**************************************************************************
**************************************************************************
**WARNING:****WARNING:****WARNING:****WARNING:****WARNING:****WARNING:**
 
*  PLEASE READ THE INSTRUCTIONS CAREFULLY AND ENTIRELY.  PLEASE FOLLOW THE
   INSTRUCTIONS EXACTLY AS THEY ARE STATED.
 
*  FAILURE TO FOLLOW INSTRUCTIONS COULD EITHER RESULT IN A DEFECTIVE BOARD OR
   UNSUCCESSFUL FLASH PROM UPDATE.
 
*  THIS IS NOT A STANDARD PATCH in that it does not use the installpatch
   and backoutpatch scripts.
 
*  THIS PATCH CANNOT BE INSTALLED ON AN ONLINE OPERATING SYSTEM BECAUSE
   THE INSTALL INSTRUCTIONS REQUIRES THAT THE SYSTEM BE BROUGHT DOWN.
   BE SURE TO SCHEDULE DOWN TIME TO INSTALL THIS PATCH.
 
*  Installation of the firmware included with this patch does NOT
   require any hardware changes if the Flash update completes normally. 
 
*  PLEASE REVIEW NOT ONLY THIS README BUT ALSO ADDITIONAL DOCUMENTATION
   GIVEN.
   The file "802-3233-xx.ps" (where xx stands for the latest numeric
   revision) is a PostScript copy of the "Sun Flash PROM Guide for Workstations
   and Workgroup Servers - Standalone Version", which  provides the following;
 
   (i) Emergency instructions in the unlikely event that the Flash
        update should fail.
 
   Note, however, that The Programming Guide was originally written for
   a user who is running the Flash PROM update utility from a bootable
   CDROM, and thus it will not contain the proper boot commands for
   installation of this patch.  Also note that the instructions in
   the document for installing packages are not valid for this patch.
 
**WARNING:****WARNING:****WARNING:****WARNING:****WARNING:****WARNING:**
**************************************************************************
**************************************************************************

README -- Last modified date:  Monday, June 21, 2004

