Remove Remote Lights Out Power Management

1. From the front of the cabinet verify that the key switches located at the bottom front of the master cabinet and any expansion cabinets are in the Standby position.

2. From the rear of the master cabinet, unscrew the three captive fasteners on the right side of the service processor and I/O panel and open the panel.

3. Locate the two DB-9 to DB-9 cables that are connected to the USB relay panel on the back of the service processor and I/O panel.

4. Disconnect the cable labeled Front Seq J14 In to the FRONT SEQ J14 connection and the cable labeled Rear Seq J14 In to the REAR SEQ J14 connection on the back of the master service panel.

   a) View the rear of the master service processor and I/O panel illustration.

5. Carefully route the ends of the cables so they don't interfere with the panel, other cables or connections. The other ends of these cables can remain connected to the front and rear power sequencers.

6. Close the service processor and I/O panel and tighten the three captive fasteners.

7. If an expansion cabinet is attached, disconnect the two 10 meter DB-9 to DB-9 expansion cabinet cables connected between the power sequencer out-jacks on the front of the master service processor and I/O panel to the power sequencer in-jacks on the front of the expansion cabinet service panel for both the front and rear power sequencers.

   a) View the connections for the expansion cabinet illustration.

8. If a second xpansion cabinet is attached, disconnect the two 10 meter DB-9 to DB-9 expansion cabinet cables connected between the power sequencer out-jacks on the front of the first expansion cabinet to the power sequencer in-jacks on the front of the second expansion cabinet service panel for both the front and rear power sequencers.

   a) View the connections for the second expansion cabinet illustration.

9. Loosen the four screws on the front key switch trim panel panel and remove the panel from the master cabinet and any expansion cabinets.

10. At the bottom front left and bottom back left of the system on the master cabinet and any expansion cabinet, press the power sequencers Local/Off/Remote switch to Local.

11. Hold the trim panel to the cabinet frame for the master cabinet and any expansion cabinets and tighten the four screws.

Disable the SW Support for Lights Out Operation

Note: SP6 is used only as an example in this procedure.

1. Establish a serial connection to the NTC.

   a) tip -9600 /dev/ttya or /dev/ttyb

   b) login: rss

   c) password: sun1rss

2. At the NTC prompt execute the following command and login to the service processor.

   a) ntc: connect local port_2

   Local protocol emulation 1.0 - Local Switch: <^[>

   b) Hit Return

   c) The following is the expected output.

   This system is for the use of authorized users only. Individuals using this computer system without authority, or in excess of their authority, are subject to having all of their activities on this system monitored and recorded by system personal. In the course of monitoring individuals improperly using this system, or in the course of system maintenance, the activities of authorized users may also be monitored. Anyone using this system expressly consents to such monitoring and is advised that if such monitoring reveals possible evidence of criminal activity, system personnel may provide the evidence of such monitoring to law enforcement officials.

3. You should now be at the sp6 console login for the service processor.

   a) sp6 console login: setup

   b) Password: !setup

   c) The following is the expected output.

   Last login: Sat Mar 6 10:20:23 from 10.0.0.27

   Mar 6 10:33:25 sp6 login: ROOT LOGIN /dev/console

   Sat Mar 6 10:33:25 MST 2004

   ***********************************************

   * StorEdge 6x20 Initial Configuration Utility *

   ***********************************************

   Select the operation you wish to perform:

   1. Initial configuration

   2. Restore previously defined configuration

   3. Unconfigure

   4. Enable SW support for Lights Out Operation

   5. Upgrade System

   Your Choice:

4. Select option number one (1) or three (3).

5. Follow the menus and update per your account specific configuration.

6. Disconnect from the service processor console login connection using the control+[ (left bracket) sequence.

   a) ^]

7. Logout of the NTC.

   a) ntc0: logout

   %Info: Connection with PORT_2 closed.

   Exiting the Lantronix SCS400

8. Disconnect from the tip session.