Remove and Replace Side Panel

1. Use an Allen wrench to loosen the four 1/4-inch shoulder screws that fasten the side panel to the cabinet frame, then remove the side panel from the cabinet frame. Repeat this step for each side panel to be removed.

   a) Use caution to not allow the side panel to fall after the last allen screw is removed.

   b) View the side panel removal illustration.

2. To replace the side panel, align the side panel screw holes to the cabinet frame screw holes.

3. Use an Allen wrench to tighten the four 1/4-inch shoulder screws to fasten the side panel to the cabinet frame.

   a) View the side panel replacement illustration.