Remove and Replace USB Flash Drive

1. Before starting this service action enable the reserve cabinet(s) function.

   a) Reserve the cabinet(s) for maintenance.

   b) Enter a description of the service action (i.e. replacing USB relay panel).

   c) Select the estimated amount of time of the service action from the pull-down.

   d) Select the Reserve button.

   e) Other users will be alerted that this service action is in progress when they log in.

2. Observe all ESD precautions.

3. From the rear of the cabinet, loosen the three captive fasteners on the right side of the Service Processor and I/O panel and open the panel.

4. Remove the USB flash drive from the rear of the service processor.

5. Insert the new USB flash drive.

6. To restore the configuration information to the new USB flash drive: restore flash drive configuration.

   a) Select the Run button from the right side of the screen.

   b) A successful completion message would be: "Backup Command Successful".

7. Close the service processor and I/O panel and tighten the three captive fasteners.

8. After this sevice action has been completed all Alarms will need to be deleted: Delete Alarms.

   a) From the left side of the screen select the "check mark" box to select all alarms.

   b) Select the Delete button to delete all of the alarms.

   Note: Be sure to delete any associated alarms from all other monitoring applications.

9. Disable the reserve cabinet(s) function.

   a) Release the cabinet(s).

   b) Select the Release button.