Monitoring the SIO Combo Card State and Network Configuration

$DEV_NAME $FRU_NAME, has been selected.

1. Before starting this service action enable the reserve cabinet(s) function.

   a) Reserve the cabinet(s) for maintenance.

   b) Enter a description of the service action (i.e. Checking the SIO combo card State and Status).

   c) Select the estimated amount of time of the service action from the pull-down.

   d) Select the Reserve button.

   e) Other users will be alerted that this service action is in progress when they log in.

2. If the correct SIO card has been selected proceed to step 3 or select another SIO card from the index on the left-side of the screen.

- Checking the State of the selected SIO Combo Card

  1. Verify the State of the SIO combo card: $DEV_NAME - $FRU_NAME.

     a) The Show Chassis screen State should be "Normal".

  2. If the SIO Combo card State is NOT "Normal" check for alarms associated to this card.

- Checking the SIO Combo Card Network Configuration and Status

  1. Display the network configuration and status of the selected SIO combo card.

     a) Display SIO combo card status.

     b) Verify the replication link addressing and status.

     c) Verify that the netmask, port enabled, default gateway and IP address configuration values are correct.

     d) Verify that the Gigabit Ethernet port values are correct.

  2. If either the SIO combo card or the network configuration information looks incorrect proceed to the SIO card removal/replacement procedures or the Diagnosing an SIO Combo Card Network Connection Problem procedures.

  3. You may also need to contact your next level of support

  4. After this sevice action has been completed all Alarms will need to be deleted: Delete Alarms.

     a) From the left side of the screen select the "check mark" box to select all alarms.

     b) Select the Delete button to delete all of the alarms.

  5. Disable the reserve cabinet(s) function.

     a) Release the cabinet(s).

     b) Select the Release button.