Removing an External Modem

1. Disconnect the external modem from the 'AUX' port of the patch panel (FIGURE 1).

- FIGURE 1 - TBS

2. Disconnect the RJ-45 cable (530-3205-01) from the 'AUX' port on the interior face of the patch panel (FIGURE 2).

- FIGURE 2 - TBS

3. Connect the RJ-45 cable (530-3205-01) to the DB-9/RJ-45 Adaptor (530-3205-01) on the Mic #2 serial port of the DSP-1000 (FIGURE 3).

- FIGURE 3 - TBS