## Setting Up Volume Verify

You can set up the Volume Verify function to run manual parity checks on Sun T3 and Sun StorEdge 6120 array volumes.

Note: Disk scrubber must be turned off for Volume Verify to be enabled.To set up the volume verify function to run on all arrays:

1. Click Sun Storage Automated Diagnostic Environment > Inventory.
   The Devices page displays summary information for each device.
2. From the Actions drop-down menu, select Set Up Volume Verify.
   The Volume Verify Setup page is displayed.
3. For the Activate Volume Verify option, select Yes.
4. To enable Volume Verify to automatically fix errors it encounters while running, select Yes for the "Run with fix option" field.
   Note: This option might mistakenly fix parity on bad blocks. Contact your storage system representative for more information.
5. From the "Run on same array at most every X days" list, select the maximum frequency, in days, with which you want Volume Verify to run on any one array.
6. From the day-of-the-week lists, choose a time period from at least one day at which that you want Volume Verify to run.
   Note: This parameter determines the scheduled start time of the volume verify function. The function may continue beyond the selected time period.
7. From the Execution Rate list, select the rate at which you want Volume Verify to run.
8. Enter the default array password, if configured, for the system.
9. Click OK.

### Related Topics

- Displaying an Exception Report for System Devices