## System Timeout Settings Page

This page displays system timeout parameters. Items marked with an asterisk (*) represent mandatory fields.

The following table describes the buttons and fields on the System Timeout Settings page.

Field | Description
*Ping | The time after which an unsuccessful `ping` attempt is considered failed.
*Email | The time after which an unsuccessful email attempt is considered failed.
*Sun Storage Arrays (HTTP tokens) | The time after which an unsuccessful receipt of Hypertext Transfer Protocol (HTTP) token data is considered failed.
*SNMP Access | The time after which an unsuccessful Simple Network Management Protocol (SNMP) access attempt is considered failed.
*Inband Discovery | The time after which an unsuccessful attempt to discover in-band devices is considered failed.
*Power Sequencer | The time after which obtaining the status of the power sequencer is considered failed.
*luxadm (Sun A5000) | The time after which an unsuccessful attempt to discover Sun A5000 devices is considered failed.
*RM6 (Sun A3500FC) | The time after which an unsuccessful attempt to discover Sun A3500FC devices is considered failed.
*sccli (Sun 3510) | The time after which an unsuccessful attempt to discover Sun 3510 devices is considered failed.

### Related Topics

- Displaying and Editing System Timeout Settings
- Resetting System Timeout Settings