Quorum Status

The Quorum Status page provides the following tables:

- Quorum Devices
- Nodes
- Vote Totals

Quorum Devices
Shared disks or slices are functionally identical to nodes in terms of quorum behavior.

Field | Description
--- | ---
Device | Qualified path of the slice or LUN configured as a quorum device.
Current Votes | Number of votes currently contributed by the quorum device.
Possible Votes | Number of possible quorum votes that the device can contribute. The number of possible votes is calculated by adding the votes for the enabled hosts to which the device is attached and subtracting 1. For example, a device is attached to two cluster nodes. The device has a possible quorum vote of (1 + 1) - 1 = 1. Disabled hosts do not contribute to the total votes.
Alarms | Provides information about any alarm that has occurred on the shared disk. For more information about alarms, see Icons and Conventions.
Status | Describes whether the device is accessible to the cluster.

Back to top

Nodes

Field | Description
--- | ---
Node | Node name.
Current Votes | Number of votes that the node is currently contributing.
Possible Votes | Maximum number of votes allocated to the node.
Alarms | Provides information about any alarm that has occurred on the node. For more information about alarms, see Icons and Conventions.
Status | Current node status.

Back to top

Totals
The Totals table shows whether the cluster can achieve quorum.
Back to top