
Installation Instructions

This document contains two sections:
A: Updating the StorageTek5320 NAS operating system software 
B: Updating the StorageTek5320 NAS RAID controller firmware

----------------------------------------------------------------

A: Updating the StorageTek5320 NAS operating system software 

It is recommended to update one cluster head at a time, enabling
service to be mainained throughout the process.

Updating Sun StorageTek 5320 Cluster NAS Software:

Start a web browser and connect to your StorageTek 5320, i.e.
  http://10.0.52.10/
(Note "Browser Requirements" below.)

Supply the administration password and click "apply".


1: In the navigation panel, select:
    > System Operations > Update Software

2. In the Update Software panel, type the path where the
   update files are located. If you need to look for the
   path, click Browse.  The update file provided with this
   patch is located in the same directory as this file.
   Look for *.IMG

3: Click the Update button and wait for the transfer of
   the system software to StorageTek 5320.

4. When the update process is complete, click no to reboot
   since this will reboot the entire cluster. 

5. Go to the "Shutdown The Server" panel, and select "Reboot This 
   Head Only". The update does not take effect until the system 
   is rebooted.

6. When the head has rebooted, it will be in Quiet Mode and the 
   other head will be in Alone Mode. You must do a recover on the
   Alone head by going to the Fault Tolerance panel, then the 
   Recover panel, and then click the Recover button.

6. When the system has recovered, repeat the complete process for the 
   other head.

Note that the system restart on the 5310 after this update
takes a few minutes longer than normal.  The additional time
is necessary for completing installation of the new software.


Browser Requirements:

[Taken from Chapter 1 of the User Guide]

To access the Web Administrator management interface, you must have
the following software:
  Windows 98/NT/2000/XP, Sun Solaris 5.7 Operating System, or Red Hat Linux
  Internet Explorer 5.5 (or later) on systems using Windows 98/NT/2000/XP
or
  NetscapeTM 4.77 (or later) on systems using Windows 98/NT/2000/XP and
  Sun Solaris Operating System. Netscape 6.0 and 6.01 are not supported.
  MozillaTM JavaTM-enabled browser with Java Plug-In 1.3.1 (or later).

----------------------------------------------------------------

B: Updating the StorageTek5320 NAS RAID controller firmware

The firmware files are included for service personel only. These are not revised 
versions and it is not necesary to install them when upgrading to this patch level. 
Installation of the img file is all that is required.

