### Responding to an IPX Diagnostic Responder Query Packet

The following list indicates the primary network components of devices that respond to an IPX Diagnostic Responder query packet:

Responding Device |  | Primary Network Components
Workstation running Novell's VLM client software |  | Component ID: 0 (IPX/SPX stack)
| Component ID: 2 (LAN driver)
|  | Component ID: 4 (Shell)
|  | Component ID: 9 (DOS application)
Workstation running Novell's 32-bit client software |  | Component ID: 0 (IPX/SPX stack)
| Component ID: 2 (LAN driver)
|  | Component ID: 4 (Shell)
|  | Component ID: 9 (DOS application)
Workstation running Microsoft's Client for NetWare Networks |  | Component ID: 0 (IPX/SPX stack)
| Component ID: 2 (LAN driver)
|  | Component ID: 4 (Shell)
intraNetWare or NetWare server |  | Component ID: 0 (IPX/SPX stack)
| Component ID: 1 (Router driver)
|  | Component ID: 6 (Server or router)
|  | Number of Local Networks = 2
NetWare MPR 3.0 or above, or an intraNetWare or NetWare server attached to multiple networks |  | Component ID: 0 (IPX/SPX stack)
| Component ID: 1 (Router driver)
| Component ID: 6 (Server or router)
|  | Number of Local Networks = 3