OBSOLETE Patch-ID# 114469-02
Keywords: XVR-4000 V880z zulu ddx window graphics
Synopsis: Obsoleted by: 114469-04 SunOS 5.8: XVR-4000 Graphics Patch
Date: Mar/06/2003

Install Requirements: None                      
Solaris Release: 8

SunOS Release: 5.8

Unbundled Product: 

Unbundled Release: 

Xref: 

Topic: 

Relevant Architectures: sun4u

BugId's fixed with this patch: 4792452 4796037 4796917 4796973 4797704 4799777 4800526 4801660 4802530 4804995 4808067 4812003

Changes incorporated in this version: 4812003 4802530 4804995 4808067 4796917

Patches accumulated and obsoleted by this patch: 

Patches which conflict with this patch: 

Patches required with this patch: 

Obsoleted by: 

Files included with this patch: 

  /usr/lib/fbconfig/SUNWzulu_config
  /usr/lib/fbconfig/sparc/libSUNWzulu_dvr.so.1
  /usr/lib/fbconfig/sparcv9/libSUNWzulu_dvr.so.1
  /usr/lib/zulu.ucode
  /usr/openwin/server/modules/ddxSUNWzulu.so.1
/platform/sun4u/kernel/drv/sparcv9/zulu

Problem Description:

4812003 zulu ddx from patch 114469-01 generates direct write errors during yoyo run
4802530 Incorrect clear pixel setting in zfb/ddx code
4804995 zuluDgaGrabDrawble sets extra bits for dga shared zfb_buf_pg[] fileds
4808067 zuluddx needs fixing for some lint errors/warnings which can cause bugs
4796917 sched context corrupted during multi stream yoyo run
 
(from 114469-01)
4796037 horizontal phase adjustment fails when doing bothlock on any separate sync  
4797704 stream b on several resolutions in doublehigh+and doublewide corrupted
4796973 driver leaves convolve #3 allocated upon svideotool exit.
4799777 Artifacts on display when viewclip is not required
4792452 Xserver doesn't start after boot up
4801660 driver emits confusing warning message when a board has a bad pipe
4800526 unsuccessful ICS clock programming could result in no video

Patch Installation Instructions:
-------------------------------- 
 
For Solaris 2.0-2.6 releases, refer to the Install.info file and/or
the README within the patch for instructions on using the generic
'installpatch' and 'backoutpatch' scripts provided with each patch.
 
For Solaris 7-8 releases, refer to the man pages for instructions on
using 'patchadd' and 'patchrm' scripts provided with Solaris.
Any other special or non-generic installation instructions should be
described below as special instructions.  The following example
installs a patch to a standalone machine:
 
	example# patchadd /var/spool/patch/104945-02
 
The following example removes a patch from a standalone system:
 
	example# patchrm 104945-02
 
For additional examples please see the appropriate man pages.

Special Install Instructions:
----------------------------- 
	After patch installation, reboot the system to load the newly
	installed driver.

README -- Last modified date:  Monday, May 19, 2003

