OBSOLETE Patch-ID# 114469-05
Keywords: xvr-4000 v880z zulu ddx window graphics
Synopsis: Obsoleted by: 114469-07 SunOS 5.8: XVR-4000 Graphics Patch
Date: Jul/08/2003


Install Requirements: Reboot after installation                      
                      
Solaris Release: 8

SunOS Release: 5.8

Unbundled Product: 

Unbundled Release: 

Xref: 

Topic: 

Relevant Architectures: sparc.sun4u

BugId's fixed with this patch: 4747098 4761925 4782193 4792452 4793942 4793943 4796037 4796917 4796973 4797704 4799777 4800526 4801660 4802530 4804995 4806680 4808067 4809512 4812003 4815925 4827241 4841825 4841963 4845198

Changes incorporated in this version: 4806680 4747098 4845198

Patches accumulated and obsoleted by this patch: 

Patches which conflict with this patch: 

Patches required with this patch: 

Obsoleted by: 

Files included with this patch: 

  /usr/lib/fbconfig/SUNWzulu_config
  /usr/lib/fbconfig/sparc/libSUNWzulu_dvr.so
  /usr/lib/fbconfig/sparc/libSUNWzulu_dvr.so.1
  /usr/lib/fbconfig/sparcv9/libSUNWzulu_dvr.so
  /usr/lib/fbconfig/sparcv9/libSUNWzulu_dvr.so.1
  /usr/lib/zulu.ucode
  /usr/openwin/server/modules/ddxSUNWzulu.so.1
/platform/sun4u/kernel/drv/sparcv9/zulu

Problem Description:

4806680 Popup Menus don't work properly in SunForum on XVR-4000
4747098 sched ctx read is unreliable
4845198 kernel panic while loading zulu microcode
 
(from 114469-04)
4841825 undefined symbol zfbEnableBS
4841963 -outputs streamA unreliable on (new) FPGA 1.0
 
(from 114469-03)
4761925 A few values of HPHASE often cause loss of genlock and hence video
4782193 Vertical stripes and ripple on monitor attached to Cadaver
4793942 Genlock is unreliable for Interlace: half a line out and not easily repaired
4793943 fbconfig's -outputs option is ignored when using a single stream
4809512 debug driver reports vrt timeouts
4815925 Zulu crash with model clipping and large polygon opt
4827241 cafe intr + hung pipe == driver deadlock
 
(from 114469-02)
4812003 zulu ddx from patch 114469-01 generates direct write errors during yoyo run
4802530 Incorrect clear pixel setting in zfb/ddx code
4804995 zuluDgaGrabDrawble sets extra bits for dga shared zfb_buf_pg[] fileds
4808067 zuluddx needs fixing for some lint errors/warnings which can cause bugs
4796917 sched context corrupted during multi stream yoyo run
 
(from 114469-01)
4796037 horizontal phase adjustment fails when doing bothlock on any separate sync
4797704 stream b on several resolutions in doublehigh+and doublewide corrupted
4796973 driver leaves convolve #3 allocated upon svideotool exit.
4799777 Artifacts on display when viewclip is not required
4792452 Xserver doesn't start after boot up
4801660 driver emits confusing warning message when a board has a bad pipe
4800526 unsuccessful ICS clock programming could result in no video

Patch Installation Instructions:
--------------------------------
 
For Solaris 2.0-2.6 releases, refer to the Install.info file and/or
the README within the patch for instructions on using the generic
'installpatch' and 'backoutpatch' scripts provided with each patch.
 
For Solaris 7-8 releases, refer to the man pages for instructions on
using 'patchadd' and 'patchrm' scripts provided with Solaris.
Any other special or non-generic installation instructions should be
described below as special instructions.  The following example
installs a patch to a standalone machine:
 
	example# patchadd /var/spool/patch/104945-02
 
The following example removes a patch from a standalone system:
 
	example# patchrm 104945-02
 
For additional examples please see the appropriate man pages.

Special Install Instructions:
-----------------------------
	After patch installation, reboot the system to load the newly
	installed driver.

README -- Last modified date:  Monday, December 15, 2003

