View Alert Log |

Note:
Alerts are actionable events. The Alert log is considerably shorter than the Event Log.

1. From the Monitor Log window, select Alert Log.
2. Customize the report by using the following pull-down menus:

- Agent Host

- Category-All is the default.
  The device types supported by the current Storage Automated Diagnostic Environment version will be displayed in the pull-down menu.

- Severity-options include All (the default), System Down, Critical (error), Alert (warning), and Caution (information).
- Event-All is the default.
  The event types supported by the current Storage Automated Diagnostic Environment version will be displayed in the pull-down menu.

- Event Type-options include All (the default), System Component Events, and System Events.

- Read the last X Kbytes from LogFile-options include 25KB (the default), 50 KB, 75KB, 100KB.
- Filter1-Type the IP address for which you want to view the Event Log into the Filter1 text box.

After you have altered each field (or accepted All as the defaults), click Search Log to produce a customized Alert Log.