OBSOLETE Patch-ID# 114608-03
Keywords: sun fire 15k hpost
Synopsis: Obsoleted by: 114608-04 SMS 1.3: hpost patch for SMS 1.3
Date: Jun/13/2003


Install Requirements: See Special Install Instructions                      
                      
Solaris Release: 8 9

SunOS Release: 5.8 5.9

Unbundled Product: System Management Services

Unbundled Release: 1.3

Xref: 

Topic: SMS 1.3: hpost patch for SMS 1.3

Relevant Architectures: sparc

BugId's fixed with this patch: 4753686 4803319 4807422 4814913 4815141 4818581 4820554 4822152 4823642 4835023 4839477 4840328 4843254 4844692 4851622 4863496

Changes incorporated in this version: 4822152 4839477 4843254 4851622 4863496

Patches accumulated and obsoleted by this patch: 

Patches which conflict with this patch: 

Patches required with this patch: 

Obsoleted by: 

Files included with this patch: 

/opt/SUNWSMS/SMS1.3/bin/hpost
/opt/SUNWSMS/SMS1.3/bin/redx
/opt/SUNWSMS/SMS1.3/lib/libxcpost.so

Problem Description:

4822152 hwad optimizations or faster SC proc will break POST
4839477 post needs to support lpost version 5.14.5
4843254 JTAG TRST not asserted low on disconnected adapter
4851622 Processor frequency setting limited to 1250Mhz
4863496 Restrict use of MaxCPU board in split expander configuration
 
(from 114608-02)
 
4753686 Domain suffers Safari Bus error during device recognition in boot process
4803319 Problems with implementation of "allow_nonX150_rated_cpu_speed"
4814913 Need to accept new Ultrasparc III+ without a warning.
4815141 Need to accept Schizo 2.4 on wPCI without warnings.
4818581 POST Domain Advanced Test timeout exceeded on some domain configurations
4820554 hpost -H hang upon lock timeout
4823642 Remove up-level warnings for XMITS 2.0
4835023 Enable checking for DX pause timeout
4840328 wfail marks wrong port's memory when no trap expected.
4844692 Add WPCI 5015694-10 Rev. 51 to stage field_ict
 
(from 114608-01)
 
4807422 Need to adjust sram dimm timing for 900 Mhz procs

Patch Installation Instructions:
--------------------------------
For Solaris 8-9 releases, refer to the man pages for instructions
on using 'patchadd' and 'patchrm' scripts provided with Solaris.
Any other special or non-generic installation instructions should be
described below as special instructions.  The following example
installs a patch to a standalone machine:
 
        example# patchadd /var/spool/patch/104945-02
 
The following example removes a patch from a standalone system:
 
        example# patchrm 104945-02
 
For additional examples please see the appropriate man pages.
 
See Also:  System Management Services (SMS) 1.3 Installation Guide 
           Part No. 816-5320-10 
           Chapter 4, SMS 1.3 Additional Software Instructions
 
           Available at: http://www.sun.com/products-n-solutions/hardware/docs/Servers/High-End_Servers/Sun_Fire_15K/SW_FW_Documentation/SMS/index.html

Special Install Instructions:
-----------------------------
 
Follow these steps when installing on the SC:
1. Record which SC is the main SC.
2. Disable failover on MAIN SC (setfailover off).
3. Stop the SMS processes on both SC's simultaneously.
        /etc/init.d/sms stop
4. Install the patch on both SC's.
5. Start the SMS processes on the previous main SC first.
        /etc/init.d/sms start
6. After all the sms processes have started (i.e. you're able to run the
   showenvironment command and get all the system's status),
   start the SMS processes on the Spare SC next.
7. Enable failover on MAIN SC (setfailover on).
 
 
Notes:
 
* When installing 114608-01 all domains must run at least a default
  level post for the fix to 4807422 to be applied.  The domains
  should undergo a setkeyswitch standby or off and then back to on.
 
* In order to get the complete fix for bugid 4839477 patch 115285-01 must be
  installed.

README -- Last modified date:  Friday, July 25, 2003

