## Array Management

Caution - Do not configure the Sun StorEdge 6000 Family arrays by using the array command-line interface and this web browser user interface at the same time. Use the command-line interface or web browser user interface.
Do not use more than one instance of the software at a time to access or configure the same storage arrays or systems. For example, two storage users using the software from two different machines cannot add the same volumes to a volume group each user is creating or modifying.

The Array Management main menu is the default page that is displayed after you log into the software. From this page, you can:

- Configure specific storage arrays
- Configure multiple arrays by duplicating an existing array's settings to another array

This page also enables you to check detailed system and device health status by launching the Storage Automated Diagnostic Environment application. (This application is installed by default on the Sun StorEdge 6300 Storage Service Processor. It must be installed on the local Solaris host for the Sun StorEdge 6100 arrays to be able to launch it from this page.)

See also Array Details and Tray Reconfiguration.

- Configuring An Array
- Managing Storage Pools
- Array Registration (Sun StorEdge 6120)
- Express Array Configuration
- Managing Profiles
- Custom Array Configuration
- Duplicating Array Settings
- Managing Volumes