Remove and Replace Rear Door

1. Open the rear door completely so it will clear the rack frame.

2. Lift the door until the door hinge pins are completely removed from the frame hinge brackets and lift it away from the unit.

3. To replace the door, have the rear door in a completely open position so it will clear the rack frame.

4. Align the top and bottom hinge pins above the frame hinge brackets and lower the door in place.

5. The door is now ready to be closed and locked.