Remove and Replace Management Interface PC Card (PCMCIA card)

1. Important: The replacement of the PCMCIA card requires special instructions, contact your next level of support on how to proceed with this procedure.

2. After contacting your next level of support enable the reserve cabinet(s) function.

   a) Reserve the cabinet(s) for maintenance.

   b) Enter a description of the service action (i.e. replacing PCMCIA card).

   c) Select the estimated amount of time of the service action from the pull-down.

   d) Select the Reserve button.

   e) Other users will be alerted that this service action is in progress when they log in.

3. Observe all ESD precautions.

4. After this sevice action has been completed all Alarms will need to be deleted: Delete Alarms.

   a) From the left side of the screen select the "check mark" box to select all alarms.

   b) Select the Delete button to delete all of the alarms.

   Note: Be sure to delete any associated alarms from all other monitoring applications.

5. After the replacement has been completed disable the reserve cabinet(s) function.

   a) Release the cabinet(s).

   b) Select the Release button.