Removing the V210 Service Processor from the Cabinet

- Press the green release tabs (top and bottom) on both sides of the service processor to release the glide rails and slide the SP until it reaches the locked position.

- Then release the inner glide rail from the locked position by pulling the trigger on the inside of the inner glide towards you on both glide rails and remove the service processor.