Remove and Replace Front Door

1. Open the front door.

2. Reach inside the door and push down on the lever attached to the spring of the top hinge pin. This causes the hinge pin to retract into the door.

3. Tilt the door out from the top mounting bracket and lift up slightly to remove the door.

4. To replace the door, tilt the door and insert the bottom hinge pin with the outside hole of the bottom left mounting bracket.

5. Reach inside the door and push down on the lever attached to the spring of the top hinge pin. This causes the hinge pin to retract into the door.

6. Align the top hinge pin with the outside hole of the top left mounting bracket.

7. Release the lever. The hinge pin extends into the mounting bracket and the door is now ready to be closed and locked.