## Volume Verify Setup Page

This page enables you to set up the volume verify feature to run on all arrays.

The following table describes the fields on the Volume Verify Setup page.

Field | Description
Activate Volume Verify | Select to enable the Volume Verify utility. Volumes are verified one at a time on a rotational basis for all enabled arrays.
Run with the fix option | Select to enable Volume Verify to automatically fix volume errors. Note: The fix option might mistakenly fix parity on bad blocks. Consult your service representative for details.
Run on same array at most every X days | Select the maximum frequency with which you want Volume Verify to run on the same array.
Sunday, Monday, Tuesday, Wednesday, Thursday, Friday, Saturday | For each day of the week on which you want Volume Verify to run, select the hour during which you want Volume Verify to run. To run Volume Verify continuously during that day, select Anytime.
Execution Rate | Select the rate at which you want Volume Verify to run on all arrays. Higher execution rates result in lower array input/output (I/O) performance.
Default Array Password | Enter the default password for arrays (if configured).

### Related Topics

- Running a Diagnostic Test on a Device
- Setting Up Volume Verify