## Configuring Remote Notification

To configure notification setup parameters:

1. Click Sun Storage Automated Diagnostic Environment > Administration > Notification.
   The Notification Setup page displays notification setup parameters.
2. Select the check box of each remote notification provider you want to enable.
3. If Network Storage Command Center (NSCC) notification is enabled, specify whether notification email to the NSCC should be encrypted.
4. If Sun StorEdge Remote Response (SSRR) notification is enabled, specify a Heartbeat Frequency for the service.
5. If Simple Network Management Protocol (SNMP) Traps is enabled, specify one or more SNMP trap recipients.
6. If Net Connect notification is enabled, specify the maximum size of Net Connect notification messages and the version of Net Connect messages to be used.
7. If the Sun Management Center (SunMC) notification is enabled, specify the IP name or IP address of the SunMC server to be notified of events and alarms and specify the frequency at which heartbeat messages are to be sent if no activity is detected.

Note: Go to the Sun Download Center (SDLC) to obtain required SunMC agent packages: `http://wwws.sun.com/software/download.`

1. Click Save.
   The configured remote notification setup parameters are saved.

### Related Topics

- About Notification
- Adding an SNMP Notification Recipient
- Editing an SNMP Notification Recipient
- Deleting an SNMP Notification Recipient
- Email Configuration Tasks
- Using Email Filters
- Editing Notification Setup Parameters