Patch-ID# 117856-19
Keywords: 6130 CSM CRM RAID network storage
Synopsis: 6130 Baseline Firmware Release (FC CSM Array Controllers)
Date: Jan/25/06

Solaris Release: 8, 9, 10

SunOS Release: 5.8, 5.9, 5.10

Unbundled Product: 6130

Unbundled Release: 1.3.1

Relevant Architectures: 6130 RAID Controllers and SBOD/SATA Expansion Modules

BugId's fixed with this patch: 

Changes incorporated in this version: 

Patches accumulated and obsoleted by this patch: 

Patches which conflict with this patch: 

Patches required with this patch: 

Obsoleted by: 

Files included with this patch: 

Problem Description: 

Patch Installation Instructions: 
-------------------------------- 
*** PRE-REQUIRED: StorEDGE 6130 Array Management Host Software v1.3 installed.
***               StorEDGE 6130 Array Firmware Upgrader patch (118185-15) 
***                   installed.

1) Login to the Management Host as "root"

2) Download/Copy this patch in your local. Uncompress them.

3) cd <patch location>

4) Install the patch

   Solaris 10:
   /usr/sbin/pkgadd -G -d <patch ID> all

   Solaris 8 & 9:
   /usr/sbin/pkgadd -d <patch ID> all

Special Install Instructions: 
----------------------------- 

1) Upgrade 6130 array using the 6130 firmware upgrader patch (118185-15).

   a) Make sure that the arrays are registered within StorADE.

          Open a browser to https://hostname:6789/
          Login to StorADE. Configure StorADE and discover 6130 array(s)

   b) cd /var/sadm/swimages/118185-15/bin

   c) To upgrade,
      ./upgrade

   d) You will be presented with a list of arrays that are out of date and
      the components that are out of date.

   e) Select the arrays to upgrade with either a space-seperated list of the
      numerals used to identify them (e.g., "1 3"), or the word 'all'.
      Upgrades of each component will take a few minutes each.  Disk I/O
      must be quiesced prior to disk drive firmware updates.

   f) Response to all warning/error displayed in Storade to get arrays' health
      back to OK.

   Firmware files are installed to the /var/sadm/swimages/117856-19/
   directory in a management host install.  Within that directory,

      CRM-F/            contains controller firmware
      CRM-F-NVSRAM/     contains controller NVSRAM
      IOM-F/            contains FC SBOD IOM firmware
      IOM-S/            contains iSATA IOM firmware
      IOM-S-CSB/        contains iSATA CSB image
      DISK/             contains disk drive firmware

2) The firmware must be downgraded first and the patch must be removed before
   uninstalling or downgrading StorEDGE 6130 Array Host Installation Software
   for Solaris.

3) To undo the previous firmware upgrade (to backout to the 6130 Host 
   Software 1.3 level:

   a) cd /var/sadm/swimages/118185-15/bin

   b) To backout,
      ./downgrade

4) To remove the patch:

   a) showrev -p | grep 117856-19
      To get the package instance.

   b) pkgrm SUNWc6130.2
      SUNWc6130.2 is the package instance obtained from step a).
