OBSOLETE Patch-ID# 117866-08

NOTE:
***********************************************************************
READ THE TERMS OF THE AGREEMENT ("AGREEMENT") IN THE LEGAL_LICENSE.TXT
FILE CAREFULLY BEFORE USING THIS SOFTWARE. BY USING THE SOFTWARE, YOU
AGREE TO THE TERMS OF THIS AGREEMENT. IF YOU DO NOT AGREE TO ALL OF THE
TERMS, PROMPTLY DESTROY THE UNUSED SOFTWARE.
***********************************************************************

Keywords: sun fire 15k hwad fomd
Synopsis: Obsoleted by: 117866-09 SMS 1.4.1: hwad libSFL fomd patch
Date: Nov/30/2005


Install Requirements: See Special Install Instructions                      
                      
Solaris Release: 8 9

SunOS Release: 5.8 5.9

Unbundled Product: System Management Services

Unbundled Release: 1.4.1

Xref: 

Topic: SMS 1.4.1:

Relevant Architectures: sparc

BugId's fixed with this patch: 4507750 4924523 4968663 5028844 5070425 5083357 6191562 6216157 6240439 6291210 6302843

Changes incorporated in this version: 6291210

Patches accumulated and obsoleted by this patch: 117403-02

Patches which conflict with this patch: 

Patches required with this patch: 

Obsoleted by: 

Files included with this patch: 

/opt/SUNWSMS/SMS1.4.1/bin/fomd
/opt/SUNWSMS/SMS1.4.1/bin/hwad
/opt/SUNWSMS/SMS1.4.1/lib/libSFL.so.1

Problem Description:

6291210 HASRAM tests occasionally fail
 
(from 117866-07)
 
6302843 hwad sending dstop events in serial causes delay and incorrect dsmd ASR
 
(from 117866-06)
 
5070425 Concurrent SMS 1.4.1 domain posts may fail with locking errors
5083357 MaxCPU processors are being reported as margined
6216157 memory leak in InterruptHandler mbox get msg flow
6240439 hPCI+ power supplies failing when margined
 
(from 117866-05)
 
5028844 Unable to retrieve board info when both SCs come up at the same time
 
(from 117866-04)
 
6191562 Change Vcore voltage from 1.225 to 1.25 volts for Jag 3.x
 
(from 117866-03)
 
4924523 dstop detected by hwad but not by dsmd
4968663 SMS needs to support Jag 3.0
 
(from 117866-02) (Patch removed from sunsolve)
 
4924523 dstop detected by hwad but not by dsmd
 
(from 117866-01)
 
4507750 Hwad takes a long time or sometimes fails to become main after restarting

Patch Installation Instructions:
--------------------------------
For Solaris 2.0-2.6 releases, refer to the Install.info file and/or
the README within the patch for instructions on using the generic
'installpatch' and 'backoutpatch' scripts provided with each patch.
 
For Solaris 7-9 releases, refer to the man pages for instructions
on using 'patchadd' and 'patchrm' scripts provided with Solaris.
Any other special or non-generic installation instructions should be
described below as special instructions.  The following example
installs a patch to a standalone machine:
 
        example# patchadd /var/spool/patch/104945-02
 
The following example removes a patch from a standalone system:
 
        example# patchrm 104945-02
 
For additional examples please see the appropriate man pages.

Special Install Instructions:
-----------------------------
 
Follow these steps when installing on the SC:
1. Record which SC is the main SC.
2. Disable failover on MAIN SC (setfailover off).
3. Stop the SMS processes on both SC's simultaneously.
        /etc/init.d/sms stop
4. Install the patch on both SC's.
5. Start the SMS processes on the previous main SC first.
        /etc/init.d/sms start
6. After all the sms processes have started (i.e. you're able to run the
   showenvironment command and get all the system's status),
   start the SMS processes on the Spare SC next.
7. Enable failover on MAIN SC (setfailover on).

README -- Last modified date:  Wednesday, March 15, 2006

