## Running a Diagnostic Test on a Device

To run a diagnostic test on a device:

1. Go to the Sun Web Console and click Storage Automated Diagnostic Environment. > Inventory.
   The Devices page displays summary information for each system device.
2. Click the component name of the device for which you want to run a diagnostic test.
   Details for the selected device are displayed.
3. Click Diagnostics.
   The Device Details page scrolls to a list of available diagnostic tests for the device.
4. Select the desired diagnostic test, and click Run Test.
   The Diagnostic Setup page is displayed for the selected diagnostic test.
   Note: When running diagnostics on the Sun StorEdge 6130 Array, both controllers must be installed and online.
5. Complete the diagnostic setup options and click Run.
   The Test Results page is displayed. Results are added when the test is completed.
   Note: Refer to the man pages for information about command line interface (CLI) diagnostic test options.

### Related Topics

- Monitoring Devices
- Reference: Array Diagnostics
- Testing an Email Address
- Recovering a Configuration
- Displaying an Exception Report for System Devices