
Installation Instructions

This document contains two sections:
A: Updating the StorageTek5320 NAS operating system software 
B: Updating the StorageTek5320 NAS RAID controller firmware

----------------------------------------------------------------

A: Updating the StorageTek5320 NAS operating system software 

This procedure is taken from the "System Maintenance" section of the:
Sun StorageTek 5320 NAS Appliance and Gateway Administration Guide


Updating Sun StorageTek 5320 NAS Software:

Start a web browser and connect to your StorageTek 5320, i.e.
  http://10.0.52.10/
(Note "Browser Requirements" below.)

Supply the administration password and click "apply".


1: In the navigation panel, select:
    > System Operations > Update Software

2. In the Update Software panel, type the path where the
   update files are located. If you need to look for the
   path, click Browse.  The update file provided with this
   patch is located in the same directory as this file.
   Look for *.IMG

3: Click the Update button and wait for the transfer of
   the system software to StorageTek 5320.

4. When the update process is complete, click Yes to reboot,
   or No to continue without rebooting. The update does not
   take effect until the system is rebooted.

Note that the system restart on the StorageTek 5320 after this 
update takes a few minutes longer than normal.  The additional 
time is necessary for completing installation of the new software.


Browser Requirements:

[Taken from Chapter 1 of the User Guide]

To access the Web Administrator management interface, you must have
the following software:
  Windows 98/NT/2000/XP, Sun Solaris 5.7 Operating System, or Red Hat Linux
  Internet Explorer 5.5 (or later) on systems using Windows 98/NT/2000/XP
or
  NetscapeTM 4.77 (or later) on systems using Windows 98/NT/2000/XP and
  Sun Solaris Operating System. Netscape 6.0 and 6.01 are not supported.
  MozillaTM JavaTM-enabled browser with Java Plug-In 1.3.1 (or later).

----------------------------------------------------------------

B: Updating the StorageTek 5320 RAID controller firmware

The firmware files are included for service personel only. These are not revised
versions and it is not necesary to install them when upgrading to this patch level.
Installation of the img file is all that is required.

