OBSOLETE Patch-ID# 121460-05

NOTE:
***********************************************************************
READ THE TERMS OF THE AGREEMENT ("AGREEMENT") IN THE LEGAL_LICENSE.TXT
FILE CAREFULLY BEFORE USING THIS SOFTWARE. BY USING THE SOFTWARE, YOU
AGREE TO THE TERMS OF THIS AGREEMENT. IF YOU DO NOT AGREE TO ALL OF THE
TERMS, PROMPTLY DESTROY THE UNUSED SOFTWARE.
***********************************************************************

Keywords: sun fire 15k hwad esmd picld chs vcmon patch
Synopsis: Obsoleted by: 121460-06 SMS 1.5: hwad esmd picld patch
Date: Jun/27/2006


Install Requirements: See Special Install Instructions                      
                      
Solaris Release: 8 9

SunOS Release: 5.8 5.9

Unbundled Product: System Management Services

Unbundled Release: 1.5

Xref: 

Topic: SMS 1.5:

Relevant Architectures: sparc

BugId's fixed with this patch: 6347023 6349997 6389622 6402229 6421799

Changes incorporated in this version: 6421799

Patches accumulated and obsoleted by this patch: 120789-04

Patches which conflict with this patch: 

Patches required with this patch: 

Obsoleted by: 

Files included with this patch: 

/opt/SUNWSMS/SMS1.5/bin/esmd
/opt/SUNWSMS/SMS1.5/bin/hwad

Problem Description:

6421799 frad calling seeprom info on MEZZX on a HPCI board ... causing hwad failure
 
(from 121460-04)
 
6402229 setkeyswitch can hang during poweron
6389622 Assigning a powered off IO board to a domain at OK prompt, a reset will power off the platform
 
(from 121460-03)
 
6389622 Assigning a powered off IO board to a domain at OK prompt, a reset will power off the platform
 
(from 121460-02)
 
6349997 ESMD reads high BBC temp during hpost
 
(from 121460-01)
 
6347023 esmd/picld coring when restarting SMS and procs are CHS disable by VCMON

Patch Installation Instructions:
--------------------------------
For Solaris 2.0-2.6 releases, refer to the Install.info file and/or
the README within the patch for instructions on using the generic
'installpatch' and 'backoutpatch' scripts provided with each patch.
 
For Solaris 7-9 releases, refer to the man pages for instructions
on using 'patchadd' and 'patchrm' scripts provided with Solaris.
Any other special or non-generic installation instructions should be
described below as special instructions.  The following example
installs a patch to a standalone machine:
 
        example# patchadd /var/spool/patch/104945-02
 
The following example removes a patch from a standalone system:
 
        example# patchrm 104945-02
 
For additional examples please see the appropriate man pages.

Special Install Instructions:
-----------------------------
 
Follow these steps when installing on the SC:
1. Record which SC is the main SC.
2. Disable failover on MAIN SC (setfailover off).
3. Stop the SMS processes on both SC's simultaneously.
        /etc/init.d/sms stop
4. Install the patch on both SC's.
5. Start the SMS processes on the previous main SC first.
        /etc/init.d/sms start
6. After all the sms processes have started (i.e. you're able to run the
   showenvironment command and get all the system's status),
   start the SMS processes on the Spare SC next.
7. Enable failover on MAIN SC (setfailover on).

README -- Last modified date:  Wednesday, July 12, 2006

