Patch-ID# 123172-03

NOTE:
***********************************************************************
READ THE TERMS OF THE AGREEMENT ("AGREEMENT") IN THE LEGAL_LICENSE.TXT
FILE CAREFULLY BEFORE USING THIS SOFTWARE. BY USING THE SOFTWARE, YOU
AGREE TO THE TERMS OF THIS AGREEMENT. IF YOU DO NOT AGREE TO ALL OF THE
TERMS, PROMPTLY DESTROY THE UNUSED SOFTWARE.
***********************************************************************

Keywords: sun fire 15k hwad coredump frad seeprom mezzx hpci xmits
Synopsis: SMS 1.6: hwad patch
Date: Jul/28/2006


Install Requirements: See Special Install Instructions                      
                      
Solaris Release: 9 10

SunOS Release: 5.9 5.10

Unbundled Product: System Management Services

Unbundled Release: 1.6

Xref: 

Topic: SMS 1.6:

Relevant Architectures: sparc

BugId's fixed with this patch: 6401382 6421799 6422690 6431238 6440021 6440591

Changes incorporated in this version: 6421799 6431238 6440021 6440591

Patches accumulated and obsoleted by this patch: 

Patches which conflict with this patch: 

Patches required with this patch: 

Obsoleted by: 

Files included with this patch: 

/etc/opt/SUNWSMS/SMS1.6/config/esmd_tuning.txt
/opt/SUNWSMS/SMS1.6/bin/esmd
/opt/SUNWSMS/SMS1.6/bin/hwad
/opt/SUNWSMS/SMS1.6/lib/libESMD.so.1
/opt/SUNWSMS/SMS1.6/lib/libI2cCommProxy.so.1
/opt/SUNWSMS/SMS1.6/lib/libPower.so.1
/opt/SUNWSMS/SMS1.6/lib/libSMSMsg.so.1

Problem Description:

6421799 frad calling seeprom info on MEZZX on a HPCI board ... causing hwad failure
6431238 hwad dies not waiting for the thrNotify threads to finish initializing, platform becomes unstable
6440021 A single D147 failure, results in board power off
6440591 secondary power supplies are not monitored on xmits
 
(from 123172-02)
 
6422690 SMS marginclock command JTAG counter value exacerbates Gchip bug
 
(from 123172-01)
 
6401382 hwad coredumps in thrIosram()

Patch Installation Instructions:
--------------------------------
For Solaris 2.0-2.6 releases, refer to the Install.info file and/or
the README within the patch for instructions on using the generic
'installpatch' and 'backoutpatch' scripts provided with each patch.
 
For Solaris 7-9 releases, refer to the man pages for instructions
on using 'patchadd' and 'patchrm' scripts provided with Solaris.
Any other special or non-generic installation instructions should be
described below as special instructions.  The following example
installs a patch to a standalone machine:
 
        example# patchadd /var/spool/patch/104945-02
 
The following example removes a patch from a standalone system:
 
        example# patchrm 104945-02
 
For additional examples please see the appropriate man pages.

Special Install Instructions:
-----------------------------
 
Follow these steps when installing on the SC:
1. Record which SC is the main SC.
2. Disable failover on MAIN SC (setfailover off).
3. Stop the SMS processes on both SC's simultaneously.
        /etc/init.d/sms stop
4. Install the patch on both SC's.
5. Start the SMS processes on the previous main SC first.
        /etc/init.d/sms start
6. After all the sms processes have started (i.e. you're able to run the
   showenvironment command and get all the system's status),
   start the SMS processes on the Spare SC next.
7. Enable failover on MAIN SC (setfailover on).

README -- Last modified date:  Friday, July 28, 2006

